ADMxxxx Run-time Installation Software
This installs software required by the Analog Devices ADMxxxx series of evaluation tools.  This for use with the following parts:
•	ADM1062 – ADM1069
•	ADM1166, ADM1168, ADM1169
•	ADM1175 – ADM1178
•	ADM1191 – ADM1192
•	ADM1275, ADM1276, ADM1075

Important Notice: I2C Interface Cables Device Drivers Requirements
The evaluation software tools for the above parts support the following USB to I2C interface cables:
•	USB-SMBUS-CABLEZ
•	USB-5PSMBUS-CABLEZ
•	USB-SDP-CABLEZ

The ADMxxxx Run-Time installs the necessary devices drivers to support these interfaces on the PC for use with the ADI evaluation tools.  These devices drivers support the Microsoft Windows XP, Vista, and 7 versions of the operating system.

If you have previously used the USB-SMBUS-CABLEZ or USB-5PSMBUS-CABLEZ with one of the following versions, or previous versions of the evaluation software, then you must also remove an older version of the device driver for these interface cables.
•	ADM106x Configuration Tool v4.0.6
•	ADM106x prog106x command line Tool v.1.0.2
•	ADM1175-8/91-92 Configuration Tool v 3.0.1

Refer to the document 'Updating USB-IIC Dongle Driver' in the Common folder of the Analog Devices entry in the Start menu for more details.

The CABLE-SMBUS-3PINZ and CABLE-SMBUS-5PINZ are Parallel port to IIC converter dongles.  These are only supported on Windows XP, due to changes in the Windows Driver architecture, it is not possible to provide support for these on any version of Windows Vista or Windows 7.

Note: While these parallel port cables are currently supported by software, users are strongly recommended to replace them with one the USB based interfaces for reliability and robustness reasons.

Minimum system requirements
Windows XP SP2
1 GHz Processor
200 Meg free disc space
512Mb RAM

Minimum viewing resolution
1024 x 768 High color (16 bit)

Version History

2.0.0 – Added support for the USB-SDP-CABLEZ.

1.0.2 - Added support for EVAL-ADM106XEBZ evaluation boards.

1.0.1 - First public release.